{"text_format":"1","workbook":"xls","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":37,"n_cols":13,"rows_kept":37,"cut":false,"hidden":false,"merged":[[36,1,36,2],[4,11,4,12],[1,1,1,12],[2,1,2,12],[4,9,4,10],[4,1,4,2]],"flags":["formulas_cached_only"]}
[]
[null,"Geschwindigkeiten"]
[null,"Kilometer/Stunde   -   Meter/Sekunde"]
[]
[null,"Basiswerte:",null,null,1,"km/h","=",0.2778,"m/sec"]
[]
[]
[null,1,"km/h","=",0.2778,"m/sec",null,null,110,"km/h","=",30.558,"m/sec"]
[null,2,"km/h","=",0.5556,"m/sec",null,null,120,"km/h","=",33.336,"m/sec"]
[null,3,"km/h","=",0.8333999999999999,"m/sec",null,null,130,"km/h","=",36.114,"m/sec"]
[null,4,"km/h","=",1.1112,"m/sec",null,null,140,"km/h","=",38.891999999999996,"m/sec"]
[null,5,"km/h","=",1.389,"m/sec",null,null,150,"km/h","=",41.67,"m/sec"]
[null,6,"km/h","=",1.6667999999999998,"m/sec",null,null,160,"km/h","=",44.448,"m/sec"]
[null,7,"km/h","=",1.9445999999999999,"m/sec",null,null,170,"km/h","=",47.226,"m/sec"]
[null,8,"km/h","=",2.2224,"m/sec",null,null,180,"km/h","=",50.004,"m/sec"]
[null,9,"km/h","=",2.5002,"m/sec",null,null,190,"km/h","=",52.782,"m/sec"]
[null,10,"km/h","=",2.778,"m/sec",null,null,200,"km/h","=",55.559999999999995,"m/sec"]
[null,15,"km/h","=",4.167,"m/sec",null,null,250,"km/h","=",69.45,"m/sec"]
[null,20,"km/h","=",5.556,"m/sec",null,null,300,"km/h","=",83.34,"m/sec"]
[null,25,"km/h","=",6.944999999999999,"m/sec",null,null,350,"km/h","=",97.23,"m/sec"]
[null,30,"km/h","=",8.334,"m/sec",null,null,400,"km/h","=",111.11999999999999,"m/sec"]
[null,35,"km/h","=",9.722999999999999,"m/sec",null,null,450,"km/h","=",125.00999999999999,"m/sec"]
[null,40,"km/h","=",11.112,"m/sec",null,null,500,"km/h","=",138.9,"m/sec"]
[null,45,"km/h","=",12.501,"m/sec",null,null,1000,"km/h","=",277.8,"m/sec"]
[null,50,"km/h","=",13.889999999999999,"m/sec",null,null,1500,"km/h","=",416.7,"m/sec"]
[null,55,"km/h","=",15.279,"m/sec",null,null,2000,"km/h","=",555.6,"m/sec"]
[null,60,"km/h","=",16.668,"m/sec",null,null,2500,"km/h","=",694.5,"m/sec"]
[null,65,"km/h","=",18.057,"m/sec",null,null,3000,"km/h","=",833.4,"m/sec"]
[null,70,"km/h","=",19.445999999999998,"m/sec",null,null,3500,"km/h","=",972.3,"m/sec"]
[null,75,"km/h","=",20.835,"m/sec",null,null,4000,"km/h","=",1111.2,"m/sec"]
[null,80,"km/h","=",22.224,"m/sec",null,null,4500,"km/h","=",1250.1,"m/sec"]
[null,85,"km/h","=",23.613,"m/sec",null,null,5000,"km/h","=",1389,"m/sec"]
[null,90,"km/h","=",25.002,"m/sec",null,null,10000,"km/h","=",2778,"m/sec"]
[null,95,"km/h","=",26.391,"m/sec",null,null,100000,"km/h","=",27780,"m/sec"]
[null,100,"km/h","=",27.779999999999998,"m/sec",null,null,1000000,"km/h","=",277800,"m/sec"]
[]
[null,"Berechnung",null,"variabel:",100,"km/h","=",100000,"m/h","=",27.77777777777778,"m/sec"]